GTKWave Tutorial

1. In gtkwave we need to add the signal to see their trace. Click on logic (1), then click on the signals (2) and drag them to the signals box (3). You can type Shift+Alt+F to zoom to best fit and then zoom in on the points of interest. If you zoom in to the right point you can see PORTB go from undefined (xx) to 00 to 0F as it goes through the initialization stages and into the main while loop. Tip: If you click on a signal and hit the left or right arrow it will go to the previous or next signal change respectively.   
   